|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Variable** | **Variable influence on process** | | | **Process influence on variables** | | |
| **Influence present? (Yes/No Description)** | **Time period/Climate domain** | **Handling of influence (How/If not - Why)** | **Influence present? (Yes/No Description)** | **Time period/Climate domain** | **Handling of influence (How/If not - Why)** |
| Temperature in bedrock | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Groundwater flow | Yes | Excavation/operation | Transport of salinity included in groundwater flow modelling (Section 3.1). Groundwater transport of other solutes not considered. | No | Excavation/operation | — |
| Temperate | Transport of salinity and reference waters included in groundwater flow modelling (Section 3.1). Flow field from hydrogeological modelling used in calculations of advective transport of radionuclides, see Section 6.1. | Temperate |
| Periglacial | Transport of salinity from beneath a permafrost layer to repository depth included in groundwater flow modelling, see Section 3.1. | Periglacial |
| Glacial | Glacial |
| Groundwater pressure | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Gas phase flow | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Repository geometry | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Fracture geometry | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Rock stresses | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Matrix minerals | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Fracture minerals | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Groundwater composition | No | Excavation/operation | — | Yes | Excavation/operation | Transport of salinity included in groundwater flow modelling, see Section 3.1. |
| Temperate | Temperate | Distribution of salinity from hydrogeology modelling. Modelling of water composition based on output from hydrogeology modelling. |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Gas composition | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Structural and stray materials | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |
| Saturation | No | Excavation/operation | — | No | Excavation/operation | — |
| Temperate | Temperate |
| Periglacial | Periglacial |
| Glacial | Glacial |